The following figures shows the results of the uniaxial simulation when with the same material parameters published in the paper.





